1. Generate Trajectory (with & without obstacle),(RRT used to generate ramps avoiding collision with obstacles)
2. Main Simulation (PID Feedback Controller 2\*3 matrix stored as a .mat file), (forward propagation with small timestep between two trajectory points),(tune PID),(point reaching threshold),(possibly 2\*6 controller or PI)
3. Car model